<!DOCTYPE qgis PUBLIC 'http://mrcc.com/qgis.dtd' 'SYSTEM'>
<qgis version="3.22.7-Bia?owie?a">
  <identifier>https://esigportal2.recife.pe.gov.br/arcgis/rest/services/Planejamento/BASES_LOTES_EDIFICACAO_BAIRRO/MapServer/3</identifier>
  <parentidentifier></parentidentifier>
  <language></language>
  <type>dataset</type>
  <title>Edificação 3D</title>
  <abstract></abstract>
  <links>
    <link url="https://esigportal2.recife.pe.gov.br/arcgis/rest/services/Planejamento/BASES_LOTES_EDIFICACAO_BAIRRO/MapServer/3" mimeType="" description="" format="" type="WWW:LINK" size="" name="fonte"/>
  </links>
  <fees></fees>
  <encoding></encoding>
  <crs>
    <spatialrefsys>
      <wkt>PROJCRS["SIRGAS 2000 / UTM zone 25S",BASEGEOGCRS["SIRGAS 2000",DATUM["Sistema de Referencia Geocentrico para las AmericaS 2000",ELLIPSOID["GRS 1980",6378137,298.257222101,LENGTHUNIT["metre",1]]],PRIMEM["Greenwich",0,ANGLEUNIT["degree",0.0174532925199433]],ID["EPSG",4674]],CONVERSION["UTM zone 25S",METHOD["Transverse Mercator",ID["EPSG",9807]],PARAMETER["Latitude of natural origin",0,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8801]],PARAMETER["Longitude of natural origin",-33,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8802]],PARAMETER["Scale factor at natural origin",0.9996,SCALEUNIT["unity",1],ID["EPSG",8805]],PARAMETER["False easting",500000,LENGTHUNIT["metre",1],ID["EPSG",8806]],PARAMETER["False northing",10000000,LENGTHUNIT["metre",1],ID["EPSG",8807]]],CS[Cartesian,2],AXIS["(E)",east,ORDER[1],LENGTHUNIT["metre",1]],AXIS["(N)",north,ORDER[2],LENGTHUNIT["metre",1]],USAGE[SCOPE["Engineering survey, topographic mapping."],AREA["Brazil - between 36°W and 30°W, northern and southern hemispheres, onshore and offshore."],BBOX[-23.8,-36,4.19,-29.99]],ID["EPSG",31985]]</wkt>
      <proj4>+proj=utm +zone=25 +south +ellps=GRS80 +towgs84=0,0,0,0,0,0,0 +units=m +no_defs</proj4>
      <srsid>2678</srsid>
      <srid>31985</srid>
      <authid>EPSG:31985</authid>
      <description>SIRGAS 2000 / UTM zone 25S</description>
      <projectionacronym>utm</projectionacronym>
      <ellipsoidacronym>EPSG:7019</ellipsoidacronym>
      <geographicflag>false</geographicflag>
    </spatialrefsys>
  </crs>
  <extent>
    <spatial dimensions="2" maxz="0" minx="279863.77199999988079071" minz="0" maxx="294325.84819999989122152" crs="EPSG:31985" maxy="9120212.69329999946057796" miny="9098104.12309999950230122"/>
  </extent>
</qgis>
